**Suggestions for Lovers Walk Maintenance/Enhancements**

|  |  |  |
| --- | --- | --- |
| **Essential/Immediate Maintenance** | **Infrastructure/Longer Term Work** | **£10K + Enhancements**  |
| 2-way traffic needs to be clearly indicated. Cut back vegetation obscuring signs & paint arrows on the road in the appropriate place  | Consider making street one way  | Create a ‘green street’ – close Lovers Walk to cars  |
| Light the steps which connect with Forth Street  | Steps – lighting, non-slip surface and build an island onto the road  | More sympathetic planting of native trees  |
| Remove the bollard on the path  | Create two lanes onto roundabout  | Clean the viewing platform at the sewage outfall.  |
| Remove or cut back trees which obscure visibility on the path  | Reposition cycle path on road and dropped kerb  | Place benches at the viewing platform  |
| Repaint the ‘SLOW’ sign on the path; currently ‘OW’ and in the wrong place  | Erect ‘cyclists give way’ sign at bridges | Create planted areas:Shady Sunny Fragranced  |
| Remove moss from area between bridges  | Create dedicated cycle/pedestrian lanes  | Place information boards at planters to inform and educate about planting choices and purposes  |
| Effective lighting under bridges  | Lower the speed limit for cars – 20/15 mph |  |
| Repair loose paving slabs at sewage outfall  | Create an exit from the ambulance depot at the Tesco traffic lights  |  |
| Paint fence  | Screen or paint the electricity substation  |  |
| Reposition lifebuoy from current position on riverbank  | Replace the fence with a uniform design  |  |
| Clean bridges and remove dead pigeons/pigeon droppings  |  |  |