**Suggestions for Lovers Walk Maintenance/Enhancements**

|  |  |  |
| --- | --- | --- |
| **Essential/Immediate Maintenance** | **Infrastructure/Longer Term Work** | **£10K + Enhancements** |
| 2-way traffic needs to be clearly indicated. Cut back vegetation obscuring signs & paint arrows on the road in the appropriate place | Consider making street one way | Create a ‘green street’ – close Lovers Walk to cars |
| Light the steps which connect with Forth Street | Steps – lighting, non-slip surface and build an island onto the road | More sympathetic planting of native trees |
| Remove the bollard on the path | Create two lanes onto roundabout | Clean the viewing platform at the sewage outfall. |
| Remove or cut back trees which obscure visibility on the path | Reposition cycle path on road and dropped kerb | Place benches at the viewing platform |
| Repaint the ‘SLOW’ sign on the path; currently ‘OW’ and in the wrong place | Erect ‘cyclists give way’ sign at bridges | Create planted areas:  Shady  Sunny  Fragranced |
| Remove moss from area between bridges | Create dedicated cycle/pedestrian lanes | Place information boards at planters to inform and educate about planting choices and purposes |
| Effective lighting under bridges | Lower the speed limit for cars – 20/15 mph |  |
| Repair loose paving slabs at sewage outfall | Create an exit from the ambulance depot at the Tesco traffic lights |  |
| Paint fence | Screen or paint the electricity substation |  |
| Reposition lifebuoy from current position on riverbank | Replace the fence with a uniform design |  |
| Clean bridges and remove dead pigeons/pigeon droppings |  |  |